Max9277 registers from Evkit init

ReadByte I2C Mode Address: 0x80 Register: 0x01 = 0x90

ReadByte I2C Mode Address: 0x80 Register: 0x02 = 0x3F

ReadByte I2C Mode Address: 0x80 Register: 0x03 = 0x00

ReadByte I2C Mode Address: 0x80 Register: 0x04 = 0x83

ReadByte I2C Mode Address: 0x80 Register: 0x05 = 0x70

ReadByte I2C Mode Address: 0x80 Register: 0x08 = 0x0B

ReadByte I2C Mode Address: 0x80 Register: 0x0C = 0x20

ReadByte I2C Mode Address: 0x80 Register: 0x0D = 0x0F

ReadByte I2C Mode Address: 0x80 Register: 0x0E = 0x02

ReadByte I2C Mode Address: 0x80 Register: 0x0F = 0x00

ReadByte I2C Mode Address: 0x80 Register: 0x10 = 0x00

ReadByte I2C Mode Address: 0x80 Register: 0x11 = 0x00

ReadByte I2C Mode Address: 0x80 Register: 0x12 = 0x00

ReadByte I2C Mode Address: 0x80 Register: 0x13 = 0xB6

ReadByte I2C Mode Address: 0x80 Register: 0x14 = 0xA0

ReadByte I2C Mode Address: 0x80 Register: 0x15 = 0x52

ReadByte I2C Mode Address: 0x80 Register: 0x17 = 0x1F

ReadByte I2C Mode Address: 0x80 Register: 0x1A = 0x00

ReadByte I2C Mode Address: 0x80 Register: 0x1B = 0x10

ReadByte I2C Mode Address: 0x80 Register: 0x1E = 0x23

ReadByte I2C Mode Address: 0x80 Register: 0x1F = 0x03